{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":2,"rows_kept":22,"flags":["formulas_cached_only"]}
[]
[null,"阴茎勃起硬度测量仪招标参数"]
["序号","招标规格参数"]
["1","可鉴别心理性与器质性勃起功能障碍。"]
["2  ","能获取阴茎勃起后的坚硬度、阴茎勃起的次数/持续时间数据。"]
["3","有夜间勃起测定仪，可连续纪录并定量分析患者在夜间自然睡眠环境下阴茎勃起的次数、持续时间、硬度、周径。"]
["4","可进行视听刺激，并实时检测阴茎勃起。"]
["5","检测的数据可实现保存、显示及打印功能。"]
["6","能监测治疗勃起功能障碍药物的有效性，指导临床用药。"]
["7","可进行病人病史的档案管理。"]
["8 ","提供的产品应是产品系列中世界上最新、最先进的产品。"]
["9","所测的结果能被国家司法部作为司法鉴定和伤残鉴定的评判依据。"]
["10","测试范围：硬度：    0%-100%. 肿胀度： 5cm-15cm."]
["11","输入：100-240V；50/60Hz;400mA"]
["12","输出：9V—1A"]
[]
[null,"阴茎勃起硬度测量仪（RigiScan ）配置清单"]
[1,"阴茎勃起硬度测量仪主机  1台"]
[2,"连接电缆                1套"]
[3,"环套                    12对"]
[4,"一次性腿部绑带          6个"]
[5,"手提箱                  1个"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}